

|  |  |  |
| --- | --- | --- |
| Item | Value | Comment |
| Start Frequency | 77GHz |  |
| Idle Time | 2us |  |
| Ramp End Time | 70.31us |  |
| ADC Valid Start Time | 1.69us | In complex 2X mode |
| ADCFs | 15MHz |  |
| IF Bandwidth | 9MHz | 0.9\*ADCFs/2 in complex 2X mode |
| NFast | 1024 |  |
| ADC Sampling Time | 68.27us | NFast/ADCFs, valid FMCW dwell time in one PRI |
| Inter Chip Time | 4.04us | Idle Time + ADC Start Time + Excess Ramping TIme |
| PRI | 72.31us | Idle Time + Ramp End Time or ADC Sampling Time + Inter Chip Time |
| Slope | 9.994MHz/us |  |
| Bandwidth | 682MHz | ADC Sampling Time \* Slope |
| Range Resolution | 0.22m |  |
| Maximum Unambiguous Range | 101.31 |  |
| NPRI | 128 |  |
| CPI | 3.784ms | NPRI \* PRI |
| Velocity Resolution | 0.515m/s or 1.854kph or 1.152mph |  |
| Maximum Unambiguous Velocity | 32.95m/s or 118.62kph or 73.708mph |  |
| Frame Periodicity | 10ms |  |